|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Clause****(e.g. 4.2.5)** | **Sub clause/Paragraph** (e.g. 4.2.5.2) | **Comments** | **Proposed change** | **Observations of the secretariat** |
| **Clause 3** |  | **Reference to test procedure is missing****4MS materials have been proven to leach less than 5 µg/l of lead into the drinking water** | **Add test procedure according to NKB4****Add: check if all metal parts comply with 4MS positive list for metals.** |  |
| **Clause 4** |  | **Define test procedure** | **Add test procedure in this paragraph** |  |
| **Clause 11** |  | **Define test procedure** | **Add test procedure according EN ISO 3822** |  |
| **Clause 13** |  | **colour marking for thermostatic mixing valves at both inlets is nor necessary, one inlet marked with colour is sufficient, according to EN 1111:2017** | **Delete last sentence.** |  |